Author: admin
Company: GeoEye

Campaign 11E-A03: Check and/or replace emissions monitoring components.

SI B18 02 12, updated in August 2012
Applies to: M57Y production Jan 2008 - Sep 2009
Inspect SCR Catalyst/Replace as required (certain part numbers)
Inspect SCR Mixer/replace as required (new design)
Inspect EGR Valve/replace as required (new design)

SI B18 02 12 - Emissions Recall Campaign 11E-A03.pdf

SI B18 01 11, September 2011
Applies to: M57Y, veh. production Sep 2009 (e90) Oct 2009 (e70).
Replace SCR Catalyst
SI B18 01 11 - SCR Replacement.pdf

SI B18 05 12, updated July 2012
Applies to: M57Y, veh. production Apr 2009-Sep 2010
Inspect/Replace SCR Mixer
Inspect/Replace EGR valve
Reprogram DDE
SI B18 05 12 - Emissions Recall 11E-A03 post April 2009.pdf

SI B11 04 12, updated June 2012
Applies to: M57Y, veh. production Jan 2010 - Mar 2011
Inspect/Replace EGR Valve/replace as required (new design)
Reprogram DDE 
SI B11 04 12 - Recall 11E-A03 Emissions.pdf

SI B18 06 12, August 2012
Applies to: M57Y, veh. production Feb 2010-Sep 2010
Replace SCR Mixer (new design)
SI B18 06 12 - Emissions Recall 11E-A03- SCR Mixer.pdf

SI B18 04 12, updated June 2012
Applies to: M57Y, veh. production Jun 2009 - Sep 2010
Replace metering unit (new design)
SI B18 04 12 - SCR Metering Replacement.pdf

SI B13 04 12, released/updated October 2012
Applies to M57Y veh. Production Nov 2009-Jul 2012
complete Vehicle code with ISTA/P 2.47.1 or later
SI B13 04 12 - Reprogram OBD for EGR & SCR Door Code 626.pdf